System requirement:
1. LabVIEW 2017 32/64bit, or later.
2. NI Vision 2017, or later.

Note:
This is just a demo for using PlayerOneCamera.lvlib for each subVI function based on LabVIEW.
The PlayerOneCamera.lvlib development based on PlayerOneCamera.dll.

Running step
1. Manual select "imgFormat"
2, Run this VI directly.
3. Change the "Exposure" and "Gain" to modify brightness.
4. Change the "Bin" to set pixel bin.
5. Change the "Format" to set image format.
6. Change the "StartX","StartY","Width","Height" to change image size.
7. Click "Stop Video" to stop live video.
8. Check "Ena Cooler" to enable cooler.
9. Change "Target Temp" to set target temperature.
10. Change "Sensor Mode" to change sensor mode if supported.
